**HMD 037 ÖN FREZELİ, BAŞ SON KESMELİ PVC KENAR BANTLAMA MAKİNASI**

|  |  |
| --- | --- |
| **TEKNİK ÖZELLİKLERİ** |  |
| **Tutkal Isınma Süresi**  | **17 Dakika** |
| *Tutkal Redüktör Devri*  | ***103 d/d***  |
| **Sıkma Kalınlığı**  | **0.40x3 mm**  |
| *Sıkma Yüksekliği* | *3x60 mm* |
| **Çalışma Hızı (Dakikada)**  | **15 m** |
| *Ön Freze Motor Gücü* | *2,2 Kw* |
| **Ön Freze Motor Devri**  | **12.000 d/d** |
| *Baş Son Kesme Motor Devri*  | *12.000 d/d* |
| **Fireze Motor Devri**  | **18.000 d/d** |
| *Elektrik Gücü*  | *11 Kw* |
| **Tutkal Kazan Hacmi**  | **3 Kg** |
| *Palet Redüktör Devri*  | *21 d/d*  |
| **Fireze Bıçağı** | **6 ağız R3** |
| *Pnömatik Bar Basıncı* | *6 ATU* |
| **Makas Kesme Kalınlığı** | **0,40 x 3 mm** |
| *Freze Temizleme Derinliği* | *0,40 x 3 mm* |
| **EBATLARI** |  |
| **Boy** | **380 cm**  |
| *Genişlik* | *80 cm*  |
| **Yükseklik** | **145 cm**  |
| *Takribi Ağırlık* | *1100 kg* |

**HMD 037 PRE-MILLING, FINE-ENDS CUTTING PVC EDGE BANDING MACHINE**

|  |  |
| --- | --- |
| **TECHNICAL PROPERTIES** |  |
| **Glue Heating Time** | **17 min.** |
| *Glue Reductor Revolution* | *103 rpm* |
| **Squeezing Thickness** | **0.40x3 mm** |
| *Squeezing Height* | *60x3 mm* |
| **Operation Speed** | **15 m Per min** |
| *Pre-Milling Motor Power* | *2.2 Kw* |
| **Pre-Milling Motor Revolution** | **12000 rpm** |
| *Head-End Cutting Motor Revolution*  | *12000 rpm* |
| **Milling Motor Revolution** | **18000 rpm**  |
| *Electrical Power* | *13 Kw* |
| **Glue Can Capacity** | **3 kg** |
| *Palette Reductor Revolution* | *21 rpm* |
| **Milling Knife** | **6 teeth R3** |
| *Pneumatic Pressure* | *6 ATU* |
| **Cutter Cutting Thickness** | **0.40x3 mm** |
| *Scraper Cleaning Depth* | *0.40x1 mm* |
| **Milling Cleaning Depth** | **0.40x3 mm** |
| **DIMENSIONS** |  |
| **Length** | **380 cm** |
| *Width* | *80 cm* |
| **Height** | **145 cm** |
| *Approx. Weight* | *1100 kg* |