**Date:**

**Offer No:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **OFFER** | | | | |
| Company: | Responsible: | | | |
| Tel: | Fax: | | E-mail: | |
| Address: | | | | |
| **Ø50 HDPE MONO FILM MACHINE 600 MM**  **GENERAL SPECIFICATIONS OF MACHINE** | | | | |
|  | | | | |
| **MODEL NAME** | | | **APM Ø50 HDPE MONO** | |
| **TOWER** | | | **FIXED TOWER 3400 MM** | |
| **SCREW DIAMETER** | | | **Ø50 BARREL** | |
| **MAXIMUM CAPACITY** | | | **55 KG** | |
| **MAX FILM WIDTH** | | | **55 CM** | |
| **MINIMUM FILM WIDTH** | | | **15 CM** | |
| **MAX. FILM THICKNESS** | | |  | |
| **MIN. FILM THICKNESS** | | |  | |
| **MAX.TOTAL ELECTRICAL POWER (MAX)** | | | **38 KW** | |
| **HEAD DIAMETER OF OUTPUT** | | | **Ø 80 MM** | |
| **DIE HEAD TYPE** | | | **MONO** | |
| **DIE HEAD SYSTEM** | | | **FIXED HEAD or ROTATION HEAD** | |
| **DIE HEAD MATERIAL** | | | **4140 NITRATED STEEL** | |
| **EMBOSSING ROLLER** | | | **EXIST** | |
| **AIR SHAFT** | | | **EXIST** | |
| **BALLOON CAGE** | | | **EXIST** | |
| **BANANA ROLLER** | | | **EXIST** | |
| **CORONA TREATMENT** | | | **OPTIONAL** | |
| **DOSING UNIT** | | | **OPTIONAL** | |
| **SPARE DIE HEAD** | | | **OPTIONAL** | |
| **ROTATING TOWER** | | | **OPTIONAL** | |
| **AUTOMATIC ABSORMENT** | | | **OPTIONAL** | |
| **CUTTING SYSTEM** | | | **OPTIONAL** | |
| **DOUBLE WINDER UNIT** | | | **OPTIONAL** | |
| **AUTOMATIC WINDER** | | | **OPTIONAL** | |

**TECHNICAL DETAILS OF MACHINE**

|  |  |
| --- | --- |
| **REDUCTOR** | **HTE 322 ‘YILMAZ’ BRAND** |
| **SCREW MATERIAL** | **1.8550 GERMAN STEEL** |
| **BARREL MATERIAL** | **1.8550 GERMAN STEEL** |
| **BARREL DIMENSION** | **Ø 50 BARREL** |
| **SCREW&BARREL PRODUCER** | **TURKEY SENMAK BRAND** |
| **BALLOON COOLING SYSTEM** | **FIXED 6 INPUT** |
| **UPPER WINDER ROLLER** | **Ø214 MM RUBBER MITHRIL TIRE COATED** |
| **WINDER ROLLER** | **Ø270 MM METAL** |
| **WINDER UNIT** | **SINGLE WINDER MANUEL** |
| **FILTER SYSTEM** | **MANUEL ROCKET SYSTEM Ø75 MM** |

**ELECTRICAL DETAILS OF MACHINE**

|  |  |
| --- | --- |
| **ROTATION HEAD MOTOR** | **0,37 kW** |
| **BALLOON COOLING MOTOR** | **2,2 KW GAMAK** |
| **BALLOON COOLING INVERTER** | **2,2 KW** |
| **BALLOON COOLING FAN** | **ALUMINIUM BODY x2 PCS** |
| **A MAIN MOTOR** | **18,5 KW GAMAK** |
| **A MAIN MOTOR INVERTER** | **18,5 KW GAMAK** |
| **B MAIN MOTOR** |  |
| **B MAIN MOTOR INVERTER** |  |
| **TAKE OFF MOTOR** | **1,5 KW GAMAK** |
| **TAKE OFF UNIT INVERTER** | **1,5 KW ABB** |
| **BARREL COOLING** | **0,75 KW 3 PCS** |
| **RESISTANCE TYPE** | **CERAMIC** |
| **WINDER MOTOR** | **1,5 KW GAMAK** |
| **WINDER INVERTER** | **1,5 KW ABB** |
| **MAIN ELECTRIC PANEL** | **ABB BRAND ALL ELECTRICAL COMPONENTS EQUIPED WITH ABB 10 INCH TOUCH SCREEN AND ALL AUTOMATION SYSTEM WILL BE MADE BY ‘GENCLER ELECTRONICS’** |







|  |  |  |  |
| --- | --- | --- | --- |
| **QNT.** | **DESCRIPTION** | **PRICE** |  |
| **1** | ***APM Ø50 HDPE MONO FILM MACHINE*** | **USD** |  |
|  | ***TOTAL PRICE*** | **USD** |  |

**1.COMMERCIAL TERMS AND CONDITION & PAYMENT TERMS**

**VAT is not included our offer.**

40% down payment upon receipt of the order confirmation

60% of the order value before shipment by TT

**2.DELIVERY TERMS**

The total price is EXW Adaplasmak Factory (according to INCOTERMS, 2010 edition)

**3. SHIPMENT TIME**

Shipment will be made approximately ... days (10 days optional) after receiving the down payment. The actual shipping date will be confirmed after your down payment is received.

In case of delay in shipment due to reasons beyond the control of Adaplasmak Plastik Makine, transportation, storage and warehouse fees to the appropriate warehouse place belong to the buyer.

**4.SUPERVISION OF INSTALLATION AND COMISSIONING**

Commissioning can be conducted by our trained personnel at the agreed time. The costs for the travel to and from the site, accommodation and expenses are belong to the buyer.

The buyer should supply personnel for the installation.

**5.WARRANTY**

We warranty for a period year (one year) following the shipping documents date of issue.

The warranty does not extend normal wear and tear, damages based on incorrect use, unsuitable operation, unsuitable facilities and chemicals.

**6.VALIDITY OF THE OFFER**

This quotation valid 1 month after the quotation date.

**Bank Details : Garati Bankası /İkitelli Siteler Branch.(USD)**

**Iban:TR45 006 2001 4400 0009 096743**

**Receiver Name: ADAPLASMAK PLASTİK MAKİNE SAN.TİC ŞTİ**