**Date:**

**OFFER No:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **OFFER** | | | | |
| Company : | Responsible: | | | |
| Tel: | Fax: | | E-mail: | |
| Address: | | | | |
| **45x55 ABA EXTRUDER 900 MM**  **GENERAL FEATURES** | | | | |
|  | | | | |
| **MACHINE CODE** | | | **APM 45X55 ABA** | |
| **TOWER** | | | **FIXED TOWER 5000 MM SINGLE FLOOR** | |
| **SCREW DIA** | | | **A-45-B50 MM BARRIER** | |
| **MAX. CAPACITY** | | | **115 KG DEPEND ON MATERIAL** | |
| **MAX FILM WIDTH** | | | **850 MM** | |
| **MIN.FILM WIDTH** | | | **200 MM** | |
| **MAX.FILM THICKNESS** | | | **SINGLE LAYER 200 MICRON** | |
| **MIN.FILM THICKNESS** | | | **SINGLE LAYER 30 MICRON** | |
| **MAX. TOTAL POWER(MAX)** | | | **55 KW** | |
| **DIE HEAD DIAMETER** | | | **85 MM** | |
| **DIE HEAD TYPE** | | | **A-B-A INTERWINDE SPIRAL** | |
| **DIE HEAD SYSTEM** | | | **FIXED** | |
| **DIE HEAD MATERIAL** | | | **4140 NITRITED STEEL** | |
| **EMBOSSING ROLLER** | | | **EXIST 1-2** | |
| **AIR SHAFT** | | | **EXIST** | |
| **BALLOON CAGE** | | | **EXIST** | |
| **BANANA ROLLER** | | | **EXIST WITH REDUCER** | |
| **CORONA** | | | **OPTIONAL** | |
| **DOSING** | | | **OPTIONAL** | |
| **SPARE DIE HEAD** | | | **OPTIONAL** | |
| **ROTATING TOWER** | | | **OPTIONAL** | |
| **RAW MATERIAL LOADER** | | | **OPTIONAL** | |
| **KNIFE SYSTEM** | | | **OPTIONAL** | |
| **DOUBLE WINDER UNIT** | | | **OPTIONAL** | |
| **AUTOMATIC WINDER** | | | **OPTIONAL** | |

**TECHNICAL SPECIFICATIONS**

|  |  |
| --- | --- |
| **REDUCER** | **HTE-322 HS-422 YILMAZ BRAND** |
| **SCREW MATERIAL** | **1.8550 NITRITED STEEL** |
| **BARREL MATERIAL** | **1.8550 GERMAN STEEL** |
| **BARREL DIAMETER** | **Ø45 Ø60(2 D) (32 D)** |
| **SCREW & BARREL PRODUCER** | **TURKISH SENMAK BRAND** |
| **BALLOON COOLING SYSTEM** | **FIXED 6 INPUT** |
| **UPPER ROLLER** | **Ø214 MM MITRIL RUBBER ROLLER** |
| **WINDER ROLLER** | **Ø270 MM STEEL** |
| **WINDER TYPE** | **SINGLE MANUAL WINDER** |
| **FILTER SYSTEM** | **MANUEL ROCKET SYSTEM Ø75 MM** |

**ELECTRICAL SPECIFICATIONS**

|  |  |
| --- | --- |
| **ROTATING DIE MOTOR** | **DOES NOT EXIST** |
| **BALLOON COOLING MOTOR** | **3 KW 1500 D/D** |
| **BALLOON COOLING INVERTER** | **3 KW ABB ACS** |
| **BALLOON COOLING FAN** | **ALUMINIUM BODY** |
| **A MAIN MOTOR** | **18,5 KW 1500 D/D** |
| **A MAIN MOTOR INVERTER** | **18,5 KW ABB 1500 D/D** |
| **B MAIN MOTOR** | **30 KW GAMAK** |
| **B MAIN MOTOR INVERTER** | **30 KW ABB ACS** |
| **UP PULLER MOTOR** | **1,5 KW 1500 D/D** |
| **UP PULLER INVERTER** | **1,5 KW ABB ACS** |
| **BARREL COOLING** | **0,75 KW 3 PCS BARREL FAN** |
| **RESISTANCES** | **CERAMIC** |
| **WINDER MOTOR** | **1,5 KW 1500 D/D** |
| **WINDER MOTOR INVERTER** | **1,5 KW ABB ACS** |
| **MAIN ELECTRIC PANEL** | **ABB BRAND AND INVERTER MATERIALS AND ABB 10 TOUCH SCREEN 'GENCLER ELECTRIC' SYSTEM WILL BE MADE BY 'GENCLER ELECTRIC'.** |









|  |  |  |  |
| --- | --- | --- | --- |
| **QNT.** | **DESCRIPTION** | **PRICE** |  |
| **1** | ***APM Ø45\*55 ABA 900 FILM MACHINE*** | **USD** |  |
|  | ***TOTAL PRICE*** |  |  |

**1.COMMERCIAL TERMS AND CONDITION & PAYMENT TERMS**

**VAT is not included our offer.**

40% down payment upon receipt of the order confirmation

60% of the order value before shipment by TT

**2.DELIVERY TERMS**

The total price is EXW Adaplasmak Factory (according to INCOTERMS, 2010 edition)

**3. SHIPMENT TIME**

Shipment will be made approximately 100 days (10 days optional) after receiving the down payment. The actual shipping date will be confirmed after your down payment is received.

In case of delay in shipment due to reasons beyond the control of Adaplasmak Plastik Makine, transportation, storage and warehouse fees to the appropriate warehouse place belong to the buyer.

**4.SUPERVISION OF INSTALLATION AND COMISSIONING**

Commissioning can be conducted by our trained personnel at the agreed time. The costs for the travel to and from the site, accommodation and expenses are belong to the buyer.

The buyer should supply personnel for the installation.

**5.WARRANTY**

We warranty for a period year (one year) following the shipping documents date of issue.

The warranty does not extend normal wear and tear, damages based on incorrect use, unsuitable operation, unsuitable facilities and chemicals.

**6.VALIDITY OF THE OFFER**

This quotation valid 1 month after the quotation date.

**Bank Details : Garati Bankası /İkitelli Siteler Branch.(USD)**

**Iban:TR45 006 2001 4400 0009 096743**

**Receiver Name: ADAPLASMAK PLASTİK MAKİNE SAN.TİC ŞTİ**