**Date:**

**Offer No:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **OFFER** | | | | |
| Company: | Responsible: | | | |
| Tel: | Fax: | | E-mail: | |
| Address: | | | | |
| **50X60 ABA EXTRUDER 1100 MM**  **GENERAL FEATURES** | | | | |
|  | | | | |
| **MACHINE CODE** | | | **APM 50X60 ABA** | |
| **TOWER** | | | **FIXED TOWER 5500 MM SINGLE LAYER** | |
| **SCREW DIA** | | | **A-50-B60 MM BARRIER** | |
| **MAX. CAPACITY** | | | **130 KG DEPEND ON MATERIAL** | |
| **MAX FILM WIDTH** | | | **1050 MM** | |
| **MIN.FILM WIDTH** | | | **300 MM** | |
| **MAX.FILM THICKNESS** | | | **SINGLE LAYER 200 MICRON** | |
| **MIN.FILM THICKNESS** | | | **SINGLE LAYER 30 MICRON** | |
| **MAX. TOTAL POWER(MAX)** | | | **67 KW** | |
| **DIE HEAD DIAMETER** | | | **100 MM** | |
| **DIE HEAD TYPE** | | | **A-B-A** | |
| **DIE HEAD SYSTEM** | | | **FIXED OZGULMAK BRAND** | |
| **DIE HEAD MATERIAL** | | | **4140 NITRITED STEEL** | |
| **EMBOSSING ROLLER** | | | **EXIST 1-2 TEETH** | |
| **AIR SHAFT** | | | **EXIST** | |
| **BALLOON CAGE** | | | **EXIST AUTOMATIC** | |
| **BANANA ROLLER** | | | **EXIST** | |
| **CORONA** | | | **OPTIONAL** | |
| **DOSING** | | | **OPTIONAL** | |
| **SPARE DIE HEAD** | | | **OPTIONAL** | |
| **ROTATING TOWER** | | | **OPTIONAL** | |
| **RAW MATERIAL LOADER** | | | **OPTIONAL** | |
| **KNIFE SYSTEM** | | | **OPTIONAL** | |
| **DOUBLE WINDING UNIT** | | | **OPTIONAL** | |
| **AUTOMATIC WINDING** | | | **OPTIONAL** | |

**TECHNICAL SPECIFICATIONS**

|  |  |
| --- | --- |
| **REDUCER** | **HS-322 HS 522 YILMAZ BRAND** |
| **SCREW MATERIAL** | **1.8550 GERMAN STEEL** |
| **BARREL MATERIAL** | **1.8550 GERMAN STEEL** |
| **BARREL DIAMETER** | **50X60** |
| **SCREW & BARREL PRODUCER** | **TURKISH SENMAK BRAND** |
| **BALLOON COOLING SYSTEM** | **FIXED 6 ENTER** |
| **UPPER ROLLER** | **Ø214 MM LASTIC STEEL** |
| **WINDING ROLLER** | **Ø270 MM STEEL** |
| **WINDING TYPE** | **SINGLE WINDER** |
| **FILTER SYSTEM** | **MANUAL ROCKET SYSTEM Ø95 MM** |

**MACHINE ELECTRICAL SPECIFICATIONS**

|  |  |
| --- | --- |
| **ROTATING DIE MOTOR** | **-** |
| **BALLOON COOLING MOTOR** | **3 kW GAMAK** |
| **BALLOON COOLING DRIVER** | **3 kW ABB** |
| **BALLOON COOLING FAN** | **ALUMINIUM BODY** |
| **A MAIN MOTOR** | **37 KW GAMAK** |
| **A MAIN MOTOR DRIVER** | **37 KW ABB** |
| **B MAIN MOTOR** | **30 KW GAMAK** |
| **B MAIN MOTOR DRIVER** | **30 KW ABB ACS** |
| **UP PULLER MOTOR** | **1,5 KW GAMAK** |
| **UP PULLER DRIVER** | **1,5 KW ABB** |
| **BARREL COOLING** | **0,75 KW 3 PCS BARREL** |
| **RESISTANCES** | **CERAMIC** |
| **WINDING MOTOR** | **1,5 KW GAMAK** |
| **WINDING MOTOR DRIVER** | **1,5 KW ABB** |
| **MAIN ELECTRIC PANEL** | **ABB BRAND AND INVERTER MATERIALS AND ABB 10 TOUCH SCREEN 'GENCLER ELECTRIC' SYSTEM WILL BE MADE BY 'GENCLER ELECTRIC'.** |





|  |  |  |  |
| --- | --- | --- | --- |
| **QNT** | **DESCRIPTION** | **PRICE** |  |
| **1** | ***APM Ø50X60 ABA EXTRUDER FILM MACHINE FIXED TOWER FIXED DIE HEAD 1100 MM*** | **USD** |  |
|  | ***TOTAL PRICE*** | **USD** |  |

**1.COMMERCIAL TERMS AND CONDITION & PAYMENT TERMS**

**VAT is not included our offer.**

40% down payment upon receipt of the order confirmation

60% of the order value before shipment by TT

**2.DELIVERY TERMS**

The total price is EXW Adaplasmak Factory (according to INCOTERMS, 2010 edition)

**3. SHIPMENT TIME**

Shipment will be made approximately 100 days (10 days optional) after receiving the down payment. The actual shipping date will be confirmed after your down payment is received.

In case of delay in shipment due to reasons beyond the control of Adaplasmak Plastik Makine, transportation, storage and warehouse fees to the appropriate warehouse place belong to the buyer.

**4.SUPERVISION OF INSTALLATION AND COMISSIONING**

Commissioning can be conducted by our trained personnel at the agreed time. The costs for the travel to and from the site, accommodation and expenses are belong to the buyer.

The buyer should supply personnel for the installation.

**5.WARRANTY**

We warranty for a period year (one year) following the shipping documents date of issue.

The warranty does not extend normal wear and tear, damages based on incorrect use, unsuitable operation, unsuitable facilities and chemicals.

**6.VALIDITY OF THE OFFER**

This quotation valid 1 month after the quotation date.

**Bank Details : Garati Bankası /İkitelli Siteler Branch.(USD)**

**Iban:TR45 006 2001 4400 0009 096743**

**Receiver Name: ADAPLASMAK PLASTİK MAKİNE SAN.TİC ŞTİ**