**Date:**

**Offer No:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **OFFER** | | | | |
| Company: | Responsible: | | | |
| Tel: | Fax: | | E-mail: | |
| Address: | | | | |
| **60x70 ABA 1300 MM EXTRUDER FILM MACHINE**  **GENERAL SPECIFICATIONS OF MACHINE** | | | | |
|  | | | | |
| **MODEL NAME** | | | **APM 60x70 ABA** | |
| **TOWER** | | | **FIXED TOWER 7000 MM DOUBLE LAYER** | |
| **SCREW DIAMETER** | | | **A-60MM- B-70MM** | |
| **MAXIMUM CAPACITY** | | | **180 KG (It depends on product)** | |
| **MAX FILM WIDTH** | | | **1250 MM** | |
| **MINIMUM FILM WIDTH** | | | **400 MM** | |
| **MAX. FILM THICKNESS** | | | **SINGLE LAYER 200 MICRON** | |
| **MIN. FILM THICKNESS** | | | **SINGLE LAYER 30 MICRON** | |
| **MAX.TOTAL ELECTRICAL POWER (MAX)** | | | **70 kW** | |
| **HEAD DIAMETER OF OUTPUT** | | | **Ø 140 MM** | |
| **DIE HEAD TYPE** | | | **A-B-A** | |
| **DIE HEAD SYSTEM** | | | **FIXED HEAD** | |
| **DIE HEAD MATERIAL** | | | **4140 NITRATED STEEL** | |
| **COFRAJ ROLLER** | | | **EXIST** | |
| **AIR SHAFT** | | | **EXIST** | |
| **BALLOON CAGE** | | | **EXIST AUTOMATIC** | |
| **BANANA ROLLER** | | | **EXIST** | |
| **CORONA TREATMENT** | | | **OPTIONAL** | |
| **DOSING UNIT** | | | **OPTIONAL** | |
| **SPARE DIE HEAD** | | | **OPTIONAL** | |
| **ROTATING TOWER** | | | **OPTIONAL** | |
| **AUTOMATIC ABSORBENT** | | | **OPTIONAL** | |
| **KNIFE SYSTEM** | | | **OPTIONAL** | |
| **DOUBLE WINDING UNIT** | | | **OPTIONAL** | |
| **AUTOMATIC WINDER** | | | **OPTIONAL** | |

**TECHNICAL DETAILS OF MACHINE**

|  |  |
| --- | --- |
| **REDUCTOR** | **HTE 522 HTE622 ‘YILMAZ’ BRAND** |
| **SCREW MATERIAL** | **1.8550 GERMAN STEEL** |
| **BARREL MATERIAL** | **1.8550 GERMAN STEEL** |
| **BARREL DIMENSION** | **60x70** |
| **SCREW&BARREL PRODUCER** | **TURKEY SENMAK BRAND** |
| **BALLOON COOLING SYSTEM** | **FIXED 6 INPUT** |
| **UPPER WINDER ROLLER** | **Ø214 MM RUBBER** |
| **WINDER ROLLER** | **Ø270 MM METAL** |
| **WINDER UNIT** | **SINGLE WINDER MANUEL** |
| **FILTER SYSTEM** | **MANUEL ROCKET SYSTEM Ø100 MM** |

**ELECTRICAL DETAILS OF MACHINE**

|  |  |
| --- | --- |
| **ROTATION HEAD MOTOR** |  |
| **BALLOON COOLING MOTOR** | **5,5 KW GAMAK** |
| **BALLOON COOLING INVERTER** | **5,5 KW ABB** |
| **BALLOON COOLING FAN** | **ALUMINIUM CHASSIS** |
| **A MAIN MOTOR** | **45 KW GAMAK** |
| **A MAIN MOTOR INVERTER** | **45 KW GAMAK** |
| **B MAIN MOTOR** | **37 kW GAMAK** |
| **B MAIN MOTOR INVERTER** | **37 kW ABB** |
| **TAKE OFF MOTOR** | **1,5 KW GAMAK** |
| **TAKE OFF UNIT INVERTER** | **1,5 KW ABB** |
| **BARREL COOLING** | **0,75 KW 3 PCS BARREL** |
| **RESISTANCE TYPE** | **CERAMIC** |
| **WINDER MOTOR** | **1,5 KW GAMAK** |
| **WINDER INVERTER** | **1,5 KW ABB** |
| **MAIN POWER PANEL** | **ABB BRAND ALL ELECTRICAL COMPONENTS EQUIPED WITH ABB 10 INCH TOUCH SCREEN AND ALL AUTOMATION SYSTEM WILL BE MADE BY ‘GENCLER ELECTRONICS’** |





|  |  |  |  |
| --- | --- | --- | --- |
| **QNT.** | **DESCRIPTION** | **PRICE** |  |
| **1** | ***APM Ø60x70 ABA EXTRUDER FILM 130MM*** | **USD** |  |
|  | ***TOTAL PRICE*** | **USD** |  |

**1.COMMERCIAL TERMS AND CONDITION & PAYMENT TERMS**

**VAT is not included our offer.**

40% down payment upon receipt of the order confirmation

60% of the order value before shipment by TT

**2.DELIVERY TERMS**

The total price is EXW Adaplasmak Factory (according to INCOTERMS, 2010 edition)

**3. SHIPMENT TIME**

Shipment will be made approximately 100 days (10 days optional) after receiving the down payment. The actual shipping date will be confirmed after your down payment is received.

In case of delay in shipment due to reasons beyond the control of Adaplasmak Plastik Makine, transportation, storage and warehouse fees to the appropriate warehouse place belong to the buyer.

**4.SUPERVISION OF INSTALLATION AND COMISSIONING**

Commissioning can be conducted by our trained personnel at the agreed time. The costs for the travel to and from the site, accommodation and expenses are belong to the buyer.

The buyer should supply personnel for the installation.

**5.WARRANTY**

We warranty for a period year (one year) following the shipping documents date of issue.

The warranty does not extend normal wear and tear, damages based on incorrect use, unsuitable operation, unsuitable facilities and chemicals.

**6.VALIDITY OF THE OFFER**

This quotation valid 1 month after the quotation date.

**Bank Details : Garati Bankası /İkitelli Siteler Branch.(USD)**

**Iban:TR45 006 2001 4400 0009 096743**

**Receiver Name: ADAPLASMAK PLASTİK MAKİNE SAN.TİC ŞTİ**