**Date:**

**Offer No:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **OFFER** | | | | |
| Company: | Responsible: | | | |
| Tel: | Fax: | | E-mail: | |
| Address: | | | | |
| **Ø70 HDPE EXTRUDER 1100 NONSTOP**  **FILM MACHINE**  **GENERAL SPECIFICATIONS OF MACHINE** | | | | |
|  | | | | |
| **MACHINE CODE** | | | **APM Ø70 HDPE** | |
| **TOWER** | | | **FIXED TOWER 7000 MM DOUBLE LAYER** | |
| **SCREW DIAMETER** | | | **Ø70 BARREL** | |
| **MAX.CAPACITY** | | | **180 KG** | |
| **MAX. FILM WIDTH** | | | **1050 mm** | |
| **MIN FILM WIDTH** | | | **250 mm** | |
| **MAX. FILM THICKNESS** | | |  | |
| **MIN. FILM THICKNESS** | | |  | |
| **MAX. TOTAL ELECTRIC POWER** | | | **60 KW** | |
| **HEAD DIAMETER OUTPUT** | | | **120 MM** | |
| **HEAD TYPE** | | | **MONO** | |
| **HEAD SYSTEM** | | | **ROTATION HEAD** | |
| **HEAD MATERIAL** | | | **4140 NITRITED STEEL** | |
| **EMBOSSING ROLLER** | | | **EXIST** | |
| **AIR SHAFT** | | | **EXIST** | |
| **BALLOON CAGE** | | | **EXIST** | |
| **BANANA ROLLER** | | | **EXIST WITH REDUCER** | |
| **CORONA TREATMENT** | | | **OPTIONAL** | |
| **DOSING UNIT** | | | **OPTIONAL** | |
| **SPARE HEAD** | | | **OPTIONAL** | |
| **ROTATION TOWER** | | | **OPTIONAL** | |
| **AUTOMATIC ABSORMENT** | | | **OPTIONAL** | |
| **KNIFE SYSTEM** | | | **OPTIONAL** | |
| **DOUBLE WINDER UNIT** | | | **OPTIONAL** | |
| **AUTOMATIC WINDER** | | | **OPTIONAL** | |


**TECHNICAL SPECIFICATIONS**


|  |  |
| --- | --- |
| **REDUCER** | **HTE 722 YILMAZ BRAND** |
| **SCREW MATERIAL** | **1.8550 GERMAN STEEL** |
| **BARREL MATERIAL** | **1.8550 GERMAN STEEL** |
| **BARREL DIAMETER** | **Ø 70 BARREL** |
| **SCREW & BARREL PRODUCER** | **TURKISH SENMAK BRAND** |
| **BALLOON COOLING SYSTEM** | **FIXED 6 INPUT** |
| **UPPER ROLLER** | **Ø214 MM NITRILE RUBBER ROLLER** |
| **WINDER ROLLER** | **Ø270 MM STEEAL COATED RUBBER** |
| **WINDER TYPE** | **SINGLE WINDER MANUAL** |
| **FILTER SYSTEM** | **MANUEL ROCKET SYSTEM Ø120 MM** |

**ELECTRICAL SPECIFICATIONS**

|  |  |
| --- | --- |
| **ROTATION DIE MOTOR** | **0,37 KW INVERTER** |
| **BALLOON COOLING MOTOR** | **5,5 KW** |
| **BALLOON COOLING INVERTER** | **5,5 KW ABB** |
| **BALLOON COOLING FAN** | **ALUMINIUM BODY** |
| **A MAIN MOTOR** | **45 KW** |
| **A MAIN MOTOR INVERTER** | **45 KW** |
| **B MAIN MOTOR** |  |
| **B MAIN MOTOR INVERTER** |  |
| **UP PULLER MOTOR** | **1,5 KW GAMAK** |
| **UP PULLER INVERTER** | **1,5 KW ABB** |
| **BARREL COOLING** | **0,75 KW 2 PCS** |
| **RESISTANCE** | **CERAMIC** |
| **WINDER MOTOR** | **1,5 KW GAMAK** |
| **WINDER INVERTER** | **1,5 KW ABB** |
| **MAIN ELECTRIC PANEL** | **ABB BRAND AND INVERTER MATERIALS AND ABB 10 TOUCH SCREEN 'GENCLER ELECTRIC' SYSTEM WILL BE MADE BY 'GENCLER ELECTRIC'.** |









|  |  |  |  |
| --- | --- | --- | --- |
| **QNT.** | **DESCRIPTION** | **PRICE** |  |
| **1** | ***APM Ø70 HDPE 1100 NONSTOP*** | **USD** |  |
|  | ***TOTAL PRICE*** | **USD** |  |

**1.COMMERCIAL TERMS AND CONDITION & PAYMENT TERMS**

**VAT is not included our offer.**

40% down payment upon receipt of the order confirmation

60% of the order value before shipment by TT

**2.DELIVERY TERMS**

The total price is EXW Adaplasmak Factory (according to INCOTERMS, 2010 edition)

**3. SHIPMENT TIME**

Shipment will be made approximately 100 days (10 days optional) after receiving the down payment. The actual shipping date will be confirmed after your down payment is received.

In case of delay in shipment due to reasons beyond the control of Adaplasmak Plastik Makine, transportation, storage and warehouse fees to the appropriate warehouse place belong to the buyer.

**4.SUPERVISION OF INSTALLATION AND COMISSIONING**

Commissioning can be conducted by our trained personnel at the agreed time. The costs for the travel to and from the site, accommodation and expenses are belong to the buyer.

The buyer should supply personnel for the installation.

**5.WARRANTY**

We warranty for a period year (one year) following the shipping documents date of issue.

The warranty does not extend normal wear and tear, damages based on incorrect use, unsuitable operation, unsuitable facilities and chemicals.

**6.VALIDITY OF THE OFFER**

This quotation valid 1 month after the quotation date.

**Bank Details : Garati Bankası /İkitelli Siteler Branch.(USD)**

**Iban:TR45 006 2001 4400 0009 096743**

**Receiver Name: ADAPLASMAK PLASTİK MAKİNE SAN.TİC ŞTİ**