**-Taş Toplama Makinası-**

**Taş Toplama Makinaları taşlı arazilerin tarıma elverişli hale getirilmesinde global tarım sektöründeki en önemli araçlardan bir tanesi haline gelmiştir.**

**-Taş toplama makinası arazilerinizdeki yüzeyden 30cm derinliğe kadar bulunan taşları yaylı elek ve özel tambur sistemiyle toplarken aynı zamanda toprağınızı işleme görevini üstlenir.**

**-Taş toplama makinası tarım arazilerinin yanı sıra sahilleri/plajları temizlemek amacıyla turizm sektörü gibi birçok endüstriyel alanda kullanılmaktadır.**

**-Ortalama 3cm'den başlayıp 45cm'e kadar çaptaki taşları toplar. Yaylı elek, yaylı tambur sistemi ve aralıklı depo sacı sayesinde toprak ve çamur toplaması yapmaz.**

**-Hardox malzeme ile uzun bıçak ömrü sunar.**

**-Güveilir özel tasarım balata/şanzıman sistemi yağ bakımları geciktrilmediği müddetçe sorun yaratmaz, uzun ömürlüdür.**

**-Kolay değiştirilebilir bıçak ve yay sistemi servis gerekmeksizin bıçak ve yay değişimine olanak sağlar.**

**-2,6m boşaltma yüksekliğine sahip tarla tipi hidrolik kaldıraçlı depo sistemi istenilen her araca ve alana boşaltım imkanı sunar.**

**-140cm, 175cm, 200cm bahçe ve tarla modellerimiz her traktöre her araziye uygun makina seçeneği sunar.**

**English;**

**-Stone Picker-**

**Stone Pickers have become one of the most important tools in the global agriculture sector in making stony lands suitable for agriculture.**

**-The stone picker picks the stones up to a depth of 30 cm from the surface of your land with a spring sieve and special drum system, while at the same time taking on the task of cultivating your soil.**

**-Stone picker machine is used in many industrial areas such as tourism sector to clean the beaches/beach as well as agricultural lands.**

**-Picks stones from 3cm to 45cm in diameter. It does not collect soil and mud thanks to the spring sieve, spring drum system and intermittent storage sheet.**

**-Provides long blade life with Hardox material.**

**-Reliable specially designed pad/gearbox system does not cause problems as long as oil maintenance is not delayed, it is long-lasting.**

**-Easy changeable blade and spring system allows blade and spring replacement without the need for service.**

**Field-type hydraulic lift tank system with a discharge height of 2.6m offers the possibility of unloading to any desired vehicle and area.**

**Our 140cm, 175cm, 200cm garden and field models offer a machine option suitable for every tractor and every terrain.**

**Teknik Özellikler;**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | **Jaguar140** | **Jaguar175** | **Jaguar200** |
| **Working depth (Max.)** | **Çalışma Derinliği (Max.)** | **30-35 cm** | **30-35 cm** | **30-35 cm** |
| **Length** | **Uzunluk** | **520 cm** | **520 cm** | **520 cm** |
| **Path width** | **Yol Genişliği** | **225 cm** | **255 cm** | **280 cm** |
| **Height** | **Yükseklik** | **255 cm** | **255 cm** | **255 cm** |
| **Working width** | **Çalışma Genişliği** | **140 cm** | **175 cm** | **200 cm** |
| **Storage height** | **Depo Yüksekliği** | **255 cm** | **255 cm** | **260 cm** |
| **Min/Max diameter of collected stones** | **Min / Max Taş Çapı** | **3 - 35 cm** | **3 - 35 cm** | **3 - 35 cm** |
| **Storage capacity** | **Depolama Kapasitesi** | **Max. 4500 kg** | **Max. 6000 kg** | **Max. 8500 kg** |
| **Required tractor power** | **Gerekli Traktör Gücü** | **50-65HP** | **60-80HP** | **80-90HP** |
| **Weight** | **Ağırlık** | **2800 kg** | **3525 kg** | **3850 kg** |
| **غربال اهتزازي مع نظام الطبل Vibrasyonlu Yaylı Elek ve Tambur Sistemi /Vibratory spring screen and drum system /** |