Taş Kırma Makinası

Taş Kırma Makinaları taşlı arazileri tarıma elverişli hale getirirken aynı zamanda toprağı mineral açıdan zenginleştirir.

-20cm çalışa derinliği; 150cm çalışma genişliğine sahip modelimiz arazilerinizdeki taşların öğütülmesini sağlar.

-Tarla, meyve bahçeleri, seralar, üzüm bağları, sahiller ve tarımdan bağımsız birçok endüstriyel alanda kullanılmaktadır.

-34 adet Elmas Karbür(Carbide) bıçakları uzun ömürlü çalışma imkanı sunar.

-Hardox şase ve gövde ile dayanıklılık maksimize edilmiş, en zorlu koşullarda dahi hatasız çalışma hedeflenmiştir.

-Özel üretim İtalyan şanzımana sahiptir.

-Balansız rotor dengesi için tesislerimizde ileri teknoloji ekipmanlar ile çalışılmaktadır.

-Tüm makinalarımız 2 yıl servis garantilidir.

English; Stone Crusher

Stone Crushers make stony lands suitable for agriculture, while enriching the soil in terms of minerals.

Our model with a working depth of 20 cm and a working width of 150 cm allows grinding the stones in your fields.

-It is used in fields, orchards, greenhouses, vineyards, beaches and many industrial areas independent of agriculture.

-34 pieces of Carbide (Carbide) blades provide long-lasting working opportunity.

Durability is maximized with Hardox chassis and body, and faultless operation is aimed even in the toughest conditions.

-It has a specially produced Italian gearbox.

-For unbalanced rotor balance, advanced technology equipments are used in our facilities.

-All our machines are guaranteed for 2 years.

|  |  |  |  |
| --- | --- | --- | --- |
| **İş genişliği** | **Working width** | **150cm** | **170 cm** |
| **Toprak işleme derinliği** | **Working depth** | **Max:20cm** | **Max. 20 cm** |
| **Çalışma hızı** | **Working speed** | **0,3-2 km/sa** | **0,3-2 km/hr** |
| **Makine ağırlığı** | **Machine weight** | **1465 kg** | **1665 kg** |
| **Makine genişliği** | **Machine width** | **178cm** | **198 cm** |
| **Makine uzunluğu** | **Machine length** | **115cm** | **115 cm** |
| **Makine yüksekliği** | **Machine height** | **130cm** | **130 cm** |
| **Kırıcı bıçak sayısı** | **Total numer of blades** | **34 adet** | **34** |
| **Kırıcı bıçak özelliği** | **Blades feature** | **Bor Karbür** | **Boron Carbide** |
| **Makine iç kaplaması** | **Machine inside coating** | **Hardox v.b.** | **Hardox** |
| **Kırıcı bıçak pozisiyonu** | **Blades position** | **Helis** | **Helix** |
| **Kuyruk mili devri** | **PTO speed** | **540d/sa** | **540 rpm** |
| **Makine arka kapak** | **Machine rear door** | **Hidrolik** | **Hydraulic** |
| **Yağ pompası güç kaynağı** | **Oil pump power supply** | **Traktör** | **Tractor** |
| **Güç gereksinimi** | **Required tractor** | **Min:80hp** | **Min. 85 HP** |
| **Gerekli traktör özelliği** | **Tractor feature** | **Süper Sürünger vites** | **Creep speeds** |
| **Garanti Süresi;** | **Warranty period** | **2 Yıl** | **2 Years** |