**Product Feature**

**Auto Air Stop Filter**

* Specially designed Auto Air Stop filter prevents the entry of air in line when the I.V. bottle is empty
* Auto Air Stop filter maintains a constant fluid level and reduces the possibility of air in the I.V. Line

**Priming Filter**

* The special Priming Filter ensures that the line fills automatically (Auto Prime) thus maintains a closed system
* Helps in reducing Healthcare Associated Infections (HAI)
* Reduces spillage and wastage of I.V. fluid

**Features and Benefits**

* Clear spike compatible with I.V. bottles
* Unique designed ring in drip chamber for secure griping
* PVC free flexible drip chamber for easy and fast priming (Drop rate 20 drops/mL)
* DEHP free tubing reduces phthalate related toxicity thus ensures Patient Safety
* Suitable for Gravity feed as well as Pressure Infusions up to 2 bars
* Also available with “Y” injection port (latex free)/ Back Check Valve
* Standard tube length: 180 cms